# Technical Data

Cordless Drill/Driver |  | GSR 18V-150 C | GSB 18V-150 C
--- | --- | --- | ---
Article number |  | ‎3 601 JJ5 0..‎ | ‎3 601 JJ5 1..‎
Rated voltage | V= | 18 | 18
Rated no-load speed n0A)
First gear | min–1 | 0–550 | 0–550
Second gear | min–1 | 0–2 200 | 0–2 200
Impact rateA) | min–1 | – | 0–30 000
Torque, hard/soft screwdriving application based on ISO 5393 (2017)A) | Nm | 100/84 | 100/84
Max. torqueA) | Nm | 150 | 150
Max. drilling diameter
Wood | mm | 150 | 150
Steel | mm | 16 | 16
Masonry | mm | − | 20
Tool holder | mm | 1.5–13 | 1.5–13
Max. screw diameter | mm | 13 | 13
WeightB) | kg | 2.4–3.5 | 2.5–3.6
Recommended ambient temperature during charging | °C | 0 to +35 | 0 to +35
Permitted ambient temperature during operation and during storage | °C | –20 to +50 | –20 to +50
Compatible rechargeable batteries |  | GBA 18V... ProCORE18V… | GBA 18V... ProCORE18V…
Recommended rechargeable batteries for maximum performance |  | ProCORE18V… ≥ 5.5 Ah | ProCORE18V… ≥ 5.5 Ah
Recommended battery chargers |  | GAL 18... GAX 18... GAL 36... | GAL 18... GAX 18... GAL 36...

A)

  Measured at 20–25 °C with rechargeable battery ProCORE18V 8.0Ah

B)

  Depends on battery in use

Values can vary depending on the product, scope of application and environmental conditions. To find out more, visit www.bosch-professional.com/wac.